# This is a Revit shared parameter file.
# Do not edit manually.
*META	VERSION	MINVERSION
META	2	1
*GROUP	ID	NAME
GROUP	1	Texte
GROUP	2	Materials and finishes
GROUP	3	Climate engineering
GROUP	4	Dimensions
GROUP	5	Others
GROUP	6	Identification data
*PARAM	GUID	NAME	DATATYPE	DATACATEGORY	GROUP	VISIBLE
PARAM	3328a800-c8c5-4068-90fe-8ca76595aba5	Drawer	TEXT		5	1
PARAM	87213901-d631-408a-bc7c-c8a6421bf1f8	Temperature_Input	HVAC_TEMPERATURE		3	1
PARAM	920bcd02-5599-479b-b823-13c2f898d7bd	Offset_Vertical	LENGTH		4	1
PARAM	4a4eb509-bcde-4555-82d8-af847ba42b7c	IfcParametre	TEXT		1	1
PARAM	c0c1df0e-242d-4bf0-8b5f-131b112a0bbd	Width_Overall	LENGTH		4	1
PARAM	f4e38810-3fcd-4d75-b84a-475e46448e21	Material_Angle	MATERIAL		2	1
PARAM	64554d11-93b9-4c4d-bf21-d6da2745f0ff	Material_Pannel	MATERIAL		2	1
PARAM	3da65516-23c3-4e68-958e-f8a1f49f9f8b	Temperature_Output	HVAC_TEMPERATURE		3	1
PARAM	f17a7320-3544-4227-9f46-60093102c059	Material_Insulation	MATERIAL		2	1
PARAM	ed5c2d21-e088-4437-b456-bd921abc5875	Material_Pipe	MATERIAL		2	1
PARAM	a86fe129-4177-4e15-a106-98319f3df89e	Weight	TEXT		6	1
PARAM	b5f6012f-aefb-4d87-9010-c6463121546e	Type_Of_Installation	TEXT		6	1
PARAM	61bd253a-8248-40c3-941c-9381e6d681d1	Pipe_Internal_Diameter	LENGTH		4	1
PARAM	cec8d052-ff9e-406f-8720-4c605c2849c9	Water_Capacity	PIPING_VOLUME		3	1
PARAM	049c525b-11f4-4c6d-9985-8c912742faad	Load_Loss	HVAC_PRESSURE		3	1
PARAM	71498f61-5ee2-4ac7-8527-82136ad6c588	Number_Pressfittings_GEBERIT_61703	INTEGER		6	1
PARAM	54911f6d-ee45-4fbb-90de-a8f3831385ae	Pipe_Thickness	LENGTH		4	1
PARAM	9f1bdb7f-1ad8-499c-a70a-65607e8d5829	Power_Delta_55°C	HVAC_POWER		3	1
PARAM	37c56e80-8c2e-4650-b05a-3f28b104dd5c	Insulation_30mm	YESNO		2	1
PARAM	2216e98a-c7a1-47b4-be1b-a29fcda29a4a	Installation_Minimal_Height	LENGTH		3	1
PARAM	0b8aa18b-454e-4e4b-bae1-6a02ba31381c	Serie	TEXT		6	1
PARAM	c782439d-7284-40bf-b8d9-818de2069116	Hanging_Position_B	LENGTH		4	1
PARAM	0d97879f-84e7-488d-a17b-987d892c0201	Water_Flow	PIPING_FLOW		3	1
PARAM	de2ca5a0-445a-4d45-8727-25d8ee4cce89	Web_Site_Builder	URL		6	1
PARAM	7d1dd6a5-f664-444e-b859-b86c6240a21f	Hanging_Position_A	LENGTH		4	1
PARAM	cd942cab-3878-44e0-8a26-72d47ebf1047	Pipe_External_Diameter	LENGTH		4	1
PARAM	f43d7bb3-fe3e-486e-9f3c-e472ca1138e2	Panel_Thickness	LENGTH		4	1
PARAM	fe42d9c4-88cf-4765-abbe-36c25eb8815e	Code	TEXT		6	1
PARAM	3d1eb5c5-62c5-4b1f-aed0-a6d712be4d8d	Temperature_Maximal_Water	HVAC_TEMPERATURE		3	1
PARAM	f9cabad7-f39b-4160-b9f1-60095f1d64d4	Temperature_Ambient	HVAC_TEMPERATURE		3	1
PARAM	7f314ae0-844d-4c5f-87dc-6db7fdce201e	Datasheet	URL		6	1
PARAM	ca01c6f3-a69f-4230-a9d4-6d7d6bfc2224	Panel_Edge_Height	LENGTH		4	1
PARAM	21a1f0f8-c3f1-4093-b7ab-ca77c9328fdb	Size	TEXT		6	1
PARAM	a7bd63f9-0c6e-4fb0-ba03-0a16d04c957c	Thermal_Power	HVAC_POWER		3	1
PARAM	0b8c07fe-c4f1-49d5-8288-c0e8fe9a5522	Choice_Of_Text_Type	FAMILYTYPE	-2000151	5	1
PARAM	312814ff-babf-4084-86b6-a3c27c8c3f88	Length_Overall	LENGTH		4	1
